MACKWORTH PROJECT ASSESSMENT FORM

DEALER INFORMATION	LIFT SYSTEM OPTIONS
Dealer Name:	Sling (Pick one style & size)	☐	Mesh	☐	X-Small	☐	Large
Address:	☐	Solid	☐	Small	☐	X-Large
☐	Supersoft	☐	Medium
City, State, Zip:
Contact Name:	Fixed Lift	☐	Manual	☐	Power
Phone:	☐	Power with Turntable
Email:
Portable	☐	CP440P
PROJECT & SHIPPING INFORMATION
Project Name:
Shipping Location:	☐	Resident	☐	Liftgate	Item MIK1 -Bottom Up/Top Down Installation Kit
☐	Dock door available	☐	Yes	☐	No
Address: Optional-If different from above
If any questions, please call (314) 889-1000

Ceiling Brackets:

55 mm Ceiling Brackets (item #1002TRKTRB55S) are used for each ceiling drop to track.

110 mm Ceiling Brackets (item #1002TRKTRB110S) are used to connect pieces of track together.

Brackets Slips (item #1002TRKTRBS) are used to lock the track into a bracket before tightening the set screw.

On straight track, use a drop every 30”.

On a 90-degree curved track, use three (item #1002TRKTRB55S) ceiling brackets.

On a 45-degree curves track, use two (item #1002TRKTRB55S) ceiling brackets.

Installation Kits:

Plan for one Installation Kit (item #MIK1) per drop bracket.

Turntables:

For all turntables, use four drops.

Track End Stops:

Track End Stops (item #1002TRKTRRWA) will be needed for each open end of track.

End Caps:

End Caps (item #1002TRKTRP) will be needed for each open end of track.

Notes:

SITE ASSESSMENT TRACK LAYOUT

Indicate location of:	Date:
Pick-up points for resident	Chargers mounted close to electric supply
Obstacles on ceiling or walls	Dimensions-point to point on track & room dimensions
Equipment such as turntables & curves